{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2,"n_cols":15,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,0,0,14]]}
["设备导入列表"]
["序号","区域名称(必填)","模型名称(必填)","设备名称(必填)","串口号","串口波特率","串口停止位","串口检测位","串口数据位","从设备ID","IP地址","端口号","MQTT主题","微功耗传感器ID","设备类型(支持开关柜\\台区\\输电线路\\杆塔)"]