{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["SCD检测功能列表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SCD检测功能列表","index":0,"n_rows":86,"n_cols":14,"rows_kept":86,"cut":false,"hidden":false,"merged":[[1,0,50,0],[51,0,58,0],[59,0,71,0],[72,0,84,0],[1,1,48,1],[51,1,55,1],[57,1,58,1],[59,1,64,1],[65,1,71,1],[72,1,78,1],[79,1,80,1],[81,1,82,1],[83,1,84,1],[1,2,3,2],[4,2,44,2],[45,2,47,2],[62,2,64,2],[1,3,3,3],[4,3,44,3],[45,3,47,3],[62,3,64,3],[4,4,6,4],[8,4,10,4],[12,4,44,4],[4,5,6,5],[8,5,10,5],[12,5,44,5],[8,6,9,6],[12,6,36,6],[37,6,42,6],[8,7,9,7],[12,7,36,7],[37,7,42,7],[12,8,22,8],[23,8,36,8],[12,9,22,9],[23,9,36,9],[8,10,11,10],[12,10,17,10],[18,10,20,10],[24,10,35,10],[15,11,17,11],[25,11,29,11]]}
["所属模块","功能","功能","描述","功能","描述","功能","描述","功能","描述","功能","功能","功能","描述"]
["检测任务 ","当前检测任务","开始检测","显示正在检测的任务名称\n、详情及结果","正在检测的任务名称"]
[{"$nulls":4},"检测详情"]
[{"$nulls":4},"检测结果"]
[null,null,"未开始检测","任务未开始检测时，可进行开\n始检测、页面区分显示待检测任务和最近检测的任务统计，待检测任务的任务状态要区分显示、最近检测任务可查看到相应任务的SCD可视化和检测结果及任务详情信息","立即开始","可点击立即开始按钮，任务进行检测，此时状态为正在检测中，且显示任务的检测详情及检测结果","正在检测中","当任务正在检测时，状态为正在\n检测中"]
[{"$nulls":6},"检测详情","检测过程中，动态加载任务\n检测的详情信息"]
[{"$nulls":6},"检测结果","显示检测任务的检测结果"]
[{"$nulls":4},"编辑模型","维护编辑模型基本信息","检测模型选择","选择模型"]
[{"$nulls":4},"待检测任务","显示待检测任务，任务状态区分显示","检测中","动态加载检测状态",null,null,"CID文件一致性校验","    上传CID文件",null,"支持上传CID文件"]
[{"$nulls":11},"      新增",null,"查看到文件进行CID校\n验后具体的区别，新增了哪些装置的详情信息"]
[{"$nulls":6},"检测","可点击检测按钮，进行检测任务",null,null,null,"      删除",null,"查看到文件进行CID校\n验后具体的区别，删除了哪些装置的详情信息"]
[{"$nulls":11},"      修改",null,"查看到文件进行CID校\n验后具体的详情的区别，修改了哪些装置信息"]
[{"$nulls":4},"最近检测任务统计-已完成","最近检测任务统计可查看到相应任务的检测结果、任务详情、SCD可视化及网络结构",{"$nulls":4},"SCD文件一致性校验","+新的对比",null,"添加新的文件进行对比"]
[{"$nulls":11},"重新对比",null,"可选择文件进行重新对比"]
[{"$nulls":11},"导出所有结果",null,"导出文件对比后的所有结果"]
[{"$nulls":11},"查看","新增","查看到文件进行SCD校\n验后具体的区别，新增了哪些装置的详情信息"]
[{"$nulls":12},"修改","查看到文件进行SCD校\n验后具体的区别，修改了哪些装置的详情信息"]
[{"$nulls":12},"删除","查看到文件进行SCD校\n验后具体的区别，删除了哪些装置的详情信息"]
[{"$nulls":10},"          SCL文件校验","导出所有结果",null,"支持导出文件进行SCL文件\n校验后的所有结果"]
[{"$nulls":11},"导出当前节点结果",null,"支持导出文件进行SCL文件\n校验后的当前节点结果"]
[{"$nulls":11},"行号点击",null,"能查看到该行号的SCD源XML"]
[{"$nulls":10},"CRC校验","校验结果选择",null,"文件进行CRC校验后，根据\n一致和不一致进行选择检验结果"]
[{"$nulls":10},"导出虚端子",null,null,"导出虚端子关系图"]
[{"$nulls":8},"SCD可视化","以电压等级区分显示装置、统计装置、可视化\n展现装置之间连接关系及详情信息置、\n可根据检索条件查询相应的装置","检索条件的搜索和筛选",null,null,"根据电压等级、间隔、装置类型进行筛选，根据IED编码和名称进行搜索"]
[{"$nulls":10},"装置的点击","装置关联关系",null,"展示装置之间输入输出关系"]
[{"$nulls":11},"输入输出控制块","关联图","展示装置输入输出控制块之间的输入输出关系图"]
[{"$nulls":12},"SV发送","展示装置sv发送的SMV端子列表详情"]
[{"$nulls":12},"SV接收","展示装置sv接收的SMV端子列表详情"]
[{"$nulls":12},"GOOSE发送","展示装置GOOSE发送的GOOSE端子列\n表详情"]
[{"$nulls":12},"GOOSE接收","展示装置GOOSE接收的GOOSE端子列\n表详情"]
[{"$nulls":11},"虚端子关系",null,"展示装置之间虚端子输入的关系图"]
[{"$nulls":11},"基础信息",null,"展示装置的数据集及装置的基本信息"]
[{"$nulls":11},"定值条目",null,"展示装置的定值条目列表详情"]
[{"$nulls":11},"信息点表",null,"展示装置的点表条目列表详情"]
[{"$nulls":11},"源文件",null,"展示装置的源文件信息"]
[{"$nulls":11},"快速搜索",null,"根据装置名称进行查找"]
[{"$nulls":10},"装置的统计",null,null,"统计具体有多少个装置"]
[{"$nulls":6},"检测结果","可查看到检测任务的检测结果，\n对检测任务的当前节点结果及\n所有结果进行导出，支持生成报告，下载报告","左侧的树形结构","检测结果以树形结构分类显示"]
[{"$nulls":8},"导出所有结果","支持导出检测任务的所有结果"]
[{"$nulls":8},"导出当前节点结果","只导出检测任务的当前节点结果"]
[{"$nulls":8},"立即生成报告","在任务检测后，可立即生成检测报告"]
[{"$nulls":8},"报告下载","下载检测报告"]
[{"$nulls":8},"行号点击","能查看到该行号的SCD源XML"]
[{"$nulls":6},"更多","查看到更多最近检测的任务"]
[{"$nulls":6},"检测任务详情","      查看到检测任务的详情信息"]
[null,null,"已完成检测","已完成检测可查看到完成任务的名称、详情及结果","完成检测的任务名称","已完成检测任务名称的显示"]
[{"$nulls":4},"检测详情","检测过程中动态加载任务检测的详情信息"]
[{"$nulls":4},"检测结果","显示检测任务的检测结果，包含装置名称、装置描述、等级、行号、描述、标准及条款"]
[null,null,"无检测任务","没有检测任\n务可添加新的检测任务","点击新建检测任务","维护新建检测任务的基本信息"]
[null,"新建检测任务",null,"维护新建检测的基本\n信息字段"]
[null,"历史任务",null,"显示历史任务详情"]
["报告结果 ","报告已生成","下载报告","下载检测任务的检测报告"]
[null,null,"导出当前节点结果","只导出检测任务的当前节点结果"]
[null,null,"导出所有结果","导出检测任务的所有检测结果"]
[null,null,"行号点击","能查看到该行号的SCD源XML信息"]
[null,null,"检查结果","以树形结构展示检测结果分类"]
[null,"报告未生成","立即生成报告","在报告还未生成时可点击立即生成报\n告按钮且成功生成检测任务的报告\n"]
[null,"报告列表","查看","查看到检测任务的检测详情，支持在\n该页面生成和下载报告以及导出结果"]
[null,null,"报告下载","下载检测报告"]
[" 基础设置  ","内置模型管理","添加间隔","维护添加间隔的基本信息字段，间隔名称、间隔类型、电压等级"]
[null,null,"勾选间隔","间隔能够成功被勾选"]
[null,null,"修改间隔","维护修改间隔的基本信息"]
[null,null,"编辑间隔模型","对装置列表、和间隔模型列表\n及关系线路列表进行管理","间隔模型列表","以树形结构展示间隔模型列表"]
[{"$nulls":4},"装置列表","以列表方式展示装置，\n每个装置可进行随意拖动"]
[{"$nulls":4},"关系线路列表","以列表方式展示关系线，\n每条关系线可进行随意拖动"]
[null,"接线方式维护","一次接线方式管理","一次接线方式管理以树形结构、分类展现"]
[null,null,"添加新分类","维护添加新分类基本信息"]
[null,null,"查看线路图","查看到线路之间的信息"]
[null,null,"查看一次接线","查看到接线的线路名称、接线方式及接线图"]
[null,null,"编辑","维护编辑一次接线基本信息"]
[null,null,"删除","删除相应的一次接线数据"]
[null,null,"间隔模型","管理间隔模型的信息、包含装置列表\n、间隔模型列表就关系线路列表"]
["系统管理   ","报告模板","新建报告模板","维护新建报告的基本信息","上传附件","实现上传附件功能，支持常用的几种格式、单个文件不超过20MB"]
[null,null,"检索条件查询","根据模板名称、日期范围进行查询"]
[null,null,"检索条件重置","重置模板名称及日期范围"]
[null,null,"勾选相应报告","勾选报告"]
[null,null,"编辑","维护编辑报告模板信息"]
[null,null,"下载","下载报告模板"]
[null,null,"删除","删除报告模板"]
[null,"系统代码管理","添加系统代码","维护添加系统代码信息"]
[null,null,"编辑系统代码","维护编辑系统代码信息"]
[null,"系统代码参数","添加系统代码参数","维护添加系统代码参数信息"]
[null,null,"编辑系统代码参数","维护编辑系统代码参数信息"]
[null,"操作日志","检索条件的查询","根据操作结果、审计分类、操作分类\n、事件类型查询"]
[null,null,"检索条件的重置","重置操作结果、审计分类、操作分类\n、事件类型"]
["登录","实现用户根据账号、密码经过验证码验证后登录系统"]